Dimensions of disk

50mm radius outer ring

15mm radius inner ring

2mm tall

I wanted each side of the lamp to be only one layer thick, so the light could easily pass through. In order to achieve this, I made the side have a thickness of 0.28mm and printed it on the Low Quality setting, which makes each layer 0.28mm thick.

I decided to use what I’d practiced earlier to make fancier looking pentagons for the lamp

<https://www.youtube.com/watch?v=22VllkNdhYg>